| # Operation Relationships by Order (tisfc1102m000) Use this session to alter the structure of the routing, that is, the sequence of operations. You can change the next operation for operations which are not Completed. Related topics Production orders - functional overview Planning production orders in SFC Production Order The production order's code. Production Order The order status of the production order. Allowed values Order Status Start Operation If the operation does not follow any other operation, this field displays an indicator for a start operation. Related topics Network routings End Operation If the operation is the final operation, this field displays an indicator for an end operation. Related topics Network routings Operation One of a series of steps in a routing that are carried out successively to produce an item. The following data is collected during a routing operation: The task. For example, sawing. The machine used to carry out the task (optional). For example, sawing machine. The place where the task is carried out (work center). For example, woodwork. The number of employees required to carry out the task. This data is used to compute order lead times, to plan production orders and to calculate cost prices. Next Operation The operation after the current operation. You can change the order of operations by editing this field. Related topics Network routings Operation Set A set of operations consecutively carried out at the same work center. Task The task that is performed in the operation. Work Center The work center where the operation is performed. Operation Status The status of the operation. |