| # Print Bill of Material (Multilevel) (tibom1411m000) Use this session to print the multilevel bill of material for items with their components at all BOM levels of the product structure. Select the items for which you want to print a BOM. Use the Configuration field to determine which BOM lines you want to print. After you click Print, you can choose from four different types of bills of material: A BOM with quantities prints BOM data that includes the operation, warehouse, length, width, number of units, inventory unit, and net quantity. A BOM with scrap prints BOM data that includes the revision, effective and expiry dates, scrap percentage and quantity, and extra information. A BOM with manufacturing data prints BOM data that includes the revision, effective and expiry dates, lead-time offset, yield aggregate plan, routing scrap aggregate plan, and whether it is a phantom. A BOM with properties prints BOM data that includes the effective and expiry dates, the effective and expiry change orders, the information whether the component items are a standard configuration, unit effective, linked to CHM or EDM, and so on. For each manufactured item, the printed multilevel bill of material displays components at all levels. Example Manufactured item: 150100 Bicycle Europe
Level | Position | Item | Description
--- | --- | --- | ---
1 | 10 | 150101 | Frame
1 | 20 | 160200 | Wheel
2 | 10 | 200135 | Spoke
2 | 20 | 200100 | Hub
3 | 10 | 210100 | Hub case
3 | 20 | 210110 | Ballbearing
The components at level 2 are used to make the item at level 1. The wheel consists of a hub and spokes. The hub case and ballbearings (level 3) are components of the hub. Use the Print Multilevel BOM (Summarized) (tibom1414m000) session, to print a summarized multilevel BOM. Use the Print Bill of Material (Single-Level) (tibom1410m000) session, to print a single-level BOM. Related topics Structure of a multilevel BOM Scrap and yield Overview of reference designators Alternative materials in BOMs Selection Range From Item An item that occurs in any module of Manufacturing. It is a purchased, manufactured, or generic item that is used in a generic/production bill of material or in a generic/production routing. To Item An item that occurs in any module of Manufacturing. It is a purchased, manufactured, or generic item that is used in a generic/production bill of material or in a generic/production routing. Configuration The configuration of the item for which you print the BOM lines. To print the BOM for a specific effectivity unit, select Specific and enter an effectivity unit. To print the BOM for the standard configuration, select Standard. To print all BOM lines, select All. Effectivity Unit A reference number on a sales order line or a sales quotation line that is used to model deviations for a unit effective item. Related topics Overview of unit effectivity Check Validity Components and Routing Against Date If this check box is selected, LN will check if the component items and routing are valid on the date indicated in the Check Validity Components and Routing Against The Date field. Check Validity Components and Routing Against Date Enter the date for which you want to check the validity of components. If the Check Validity Components and Routing Against The Date check box is selected, you can enter a date. Print COLT Details If this check box is selected, information about cumulative order lead times (COLT) is printed on the report. Also information about noncritical COLT and other lead times is included. This information can help the planner to ensure that the order planning horizons and the master planning horizons are sufficient. Related topics Cumulative order lead times and horizons Options Print Product Variant Options If this check box is selected, the options for the product variant are printed. Print Material-Routing Relations If this check box is selected, any material-routing relationships for the component items are printed. Material-routing relationships are defined in the BOM Line - Material-Routing Relationships (tibom0140m000) session. Print Operation Texts If this check box is selected, any texts created in the Routing Operations (tirou1102m000) session are printed. To create or edit these texts: Start the Routing Operations (tirou1102m000) session. Double-click an operation. Click the Text button. Note You can not select this check box unless the Print Operations check box is also selected. Alternative Material If this check box is selected, the alternative materials that are linked to the BOM are printed in the report. Related topics Alternative materials in BOMs Explode Purchased BOMs If this check box is selected, LN also prints the BOM structures for items of type Purchased. Print Operations If this check box is selected, the routing operations for each component item are printed. Print BOM Texts If this check box is selected, then any texts linked to the bill of material will be printed. You can create or edit a text: Start the Bill of Material (tibom1110m000) session. Double-click a component item. Click the Text button. Use Up Material If this check box is selected, the use-up materials that are linked to the BOM are printed in the report. Related topics Using up remaining stock of outdated items Print Item Texts If this check box is selected, then any texts associated with items will be printed. To create or edit item text: Start the Items - General (tcibd0501m000) session. Double click an item. Click the Text button. Reference Designator If this check box is selected, the reference designators that are linked to the BOM are printed in the report. Related topics Overview of reference designators Text Language Enter the code for the language in which you want to print the texts that you have previously selected. If none of the check boxes for printing texts are selected, you cannot enter a code. |