| Print EBOM and PBOM Consistency (tiedm1470m000) |  |
| Use this session to print any differences between the engineering bills of material (EBOMs) and production bills of material (PBOMs). The differences can be the result of changes applied to either the EBOM or to the PBOM, after the EBOM has been copied to the PBOM. ERP LN only checks differences between data that has been copied from an EBOM and the PBOM, not other changes to PBOM. ERP LN checks four questions: Is there any difference between a line of the PBOM copied from the EBOM and the corresponding line of the EBOM (including deletion of the EBOM line)? Have any lines been added to the EBOM, but not to the PBOM? It is not possible to change the EBOM after the revision has been approved. Only exceptions can be modified. Have any PBOM lines been removed? Are there any differences between the line of the EBOM copy data and the line of the PBOM in the following fields? Main Item Sequence Number Exceptions Related topics Engineering data management summary Copying E-items to items Engineering BOMs Structure of a single-level BOM To print a document or a report To use From and To fields
Fields | Description
From Engineering Item | The source E-item. Related topics Engineering item
To Engineering Item | The source E-item. Related topics Engineering item
Engineering Item Revision | The source E-item revision. Related topics Engineering item revision
Revision | The source E-item revision. Related topics Engineering item revision
From Main Item | The target item. Related topics Item
To Main Item | The target item. Related topics Item To use From and To fields
Differences Only | Select this check box if you want your report to show only the BOMs which differ between EBOM and production BOM.