| Line Segment - Line Rules (tiasl1571m000) |  |
| Use this session to view the rules that are linked to a particular line segment. On the Specific menu, you can choose to see all the line rules for the line segment or only the current line rules. In Line Assembly Control (LAC), you can link several rules, each of which is valid for a different date range. You can also link more than one rule to the same segment for the same date range. In that case, if there is a contradiction, the rule with the highest priority takes precedence. You can define rules in the Line Rules (tiasl1570m000) session, or in your configurator package. Related topics Assembly control overview Line sequencing and rule types in Assembly Control
Fields | Description
Line Segment | A set of consecutive assembly-line work centers on an assembly line between two buffers. The first buffer is the beginning of the segment, the next buffer is the first part of the next segment.
Rule | Logical condition determining action.
Rule | Logical condition determining action.
Effective Date | The earliest date when the rule can be used.
Expiry Date | The last date when the rule can be used.