| To set up inspection methods for end products |  |
| To set up inspection methods for end products If the QMS Implemented for Production (SFC) check box in the Quality Management Parameters (qmptc0100m000) session has been selected, you can use Quality Management to check the end products of production orders. You can define the quality requirements for each manufactured item in Quality Management. If you select the Production (SFC) Order-Specific Inspection Data check box in the Quality Management Parameters (qmptc0100m000) session, you can zoom to the Specific Orders - By Origin (qmptc0149m000) session from the Production Orders (tisfc0501m000) session. You can choose between two methods which determine the interactions between the Shop Floor Control module and the Quality Management package with respect to the end products: The products are inspected, but the inspection orders have no direct effect on the production orders (method A). You must inspect the products before you can report a production order completed. However, you are free to report any quantity to deliver or quantity rejected, regardless of the results of the tests (method B). The Blocking Method for Inspections field in the Standard Orders - by Origin (qmptc1120m000) session determines which of the methods mentioned above will be used. ERP LN applies method A, if the Blocking Method for Inspections field has the Continue value. ERP LN applies method B, if the Blocking Method for Inspections field has the Block value. ERP LN will determine the value of these fields on the basis of the data you enter in the following sessions: Quality Combinations (qmptc0111m000) Specific Orders - By Origin (qmptc0149m000) Related topics Using QM for manufacturing operations Using QM for products of production orders Using QM for materials of production orders |