| Generate Machine Input/Output Control Data (tisfc3220m000) |  |
| Use this session to generate the input/output data for a range of machines. The data ERP LN generates is determined by the following fields in the Shop Floor Control Parameters (tisfc0100s000) session: Update Method I/O Control: determines whether the target period is a number of weeks or a number of days. No. of Periods to Generate I/O Data: determines how many days or weeks the target period contains. Include Partial Completions (Default): determines whether or not ERP LN must take into account routing operations that are only partially completed to calculate input / output values. Related sessions You can delete data which you no longer require with the Delete Machine Input/Output Control (tisfc3222m000) session. You can generate input/output data for work centers with the Generate Work Center Input/Output Control (tisfc3210m000) session. Related topics Input / output control
Fields | Description
Machine | The first of a range of machines for which you want to calculate the input/output data.
Machine | The last of a range of machines for which you want to calculate the input/output data.
Include Partial Completions (Default) | If this check box is selected, ERP LN also takes into account the routing operations that are only partially reported completed to calculate the input/output values. If this check box is cleared, ERP LN only takes into account the routing operations that are entirely reported completed to calculate the input/output values. You can set the default value for the Include Partial Completions (Default) check box in the Shop Floor Control Parameters (tisfc0100s000) session.