| Specific Orders - By Origin (qmptc0149m000) |  |
| Use this session to list, modify, or delete order-specific inspections. This session displays the numbers of the orders in other ERP LN modules for which a quality combination and/or order-specific inspection data exists. You can also enter new order-specific data manually for orders without a quality combination. If a quality combination for an origin/item combination exists, the order-specific inspection data is by default filled by the quality combination data. If you select Order Specific Inspection Data from the Specific menu, you can display or maintain the inspection data for the origin orders. Note You can only make order-specific inspections if you select one or more Order-Specific Inspection Data check boxes in the Quality Management Parameters (qmptc0100m000) session. These parameters indicate, per origin, whether or not order-specific inspection data can be defined for a specific origin order. Related topics Order-specific inspections
Fields | Description
Origin | An integrated module or package to which an (inspection) order is related.
Order | The order number of the order for which inspection is needed.
Position | The position number on the order to which the inspection order is linked. This can be the position number of the sales order line, the position number of the purchase order line, or the position number in the BOM.
Operation | One of a series of steps in a routing that are carried out successively to produce an item. The following data is collected during a routing operation: The task. For example, sawing. The machine used to carry out the task (optional). For example, sawing machine. The place where the task is carried out (work center). For example, woodwork. The number of employees required to carry out the task. This data is used to compute order lead times, to plan production orders and to calculate cost prices. A quality inspection must take place, during or after this operation.
QM Only Recommends | This field is used to indicate what can be done with the inspection results. Allowed values If this check box is selected, the inspection results are a recommendation for the user; the user can overwrite these results. If this check box is cleared, the inspection results are mandatory; the user cannot overwrite these results. In this case you cannot use destructive tests. Note This field overrules the value of the QM Only Recommends field in the Quality Management Parameters (qmptc0100m000) session.
Blocking Method for Inspections | The blocking method refers to the way in which production, purchase, or sales, is stopped or controlled in order to carry out inspections.
Commands | Description
Print Order-specific Inspection Data | Starts the Print Order-specific Inspection Data (qmptc0450m000) session.
Global Update | Starts the Global Update of Order-Specific Inspection Data (qmptc0250m000) session.
Inspection Orders | Starts the Specific Order - Inspection Orders (qmptc0150m000) session.