| Backflushing in jobs |  |
| If the Backflushing Method field in the Shop Floor Control Parameters (tisfc0100s000) session is Automatic, backflushing is performed every time a quantity is reported as complete. If you select Interactive, you can choose whether to perform backflushing after a quantity is completed. If the Backflushing Method field is Manual, to backflush material use the Backflush Materials and Hours (tisfc0220m000) session . If you select the Completed Operations Only check box, backflushing is only performed after an operation is completed, instead of after every completed quantity. If you create a job, you can perform backflushing during the off hours. Performance aspects Effect on CPU: Yes Effect on database growth: Yes Related topics Backflushing |