| # Line Station Variant - Operations (tiasc2122m000) Use this session to view and add or modify the operations associated with a line-station variant. You can only modify order-specific LSVs. For details, see the online manual topic on Line station variants and line station orders. From the appropriate menu, you can start the Line Station Variant - Assembly Parts (tiasc2121m000) session to display the parts assigned to the line-station variant. Note You cannot change the content of LSV-Assembly Parts for an order-specific line station variant if the hours for the line station order are already backflushed. Related topics Line station variants and line station orders Line Station Variant Holds identical operations and materials that are used at a specific line station for multiple assembly orders. In this manner, the identical operations and materials are stored only once, rather than for each assembly order. When line station variants are used, less data storage is required, and the performance is enhanced. Example You produce cars with various features, including two types of wheels: broad and narrow. In the wheel line station, in which the wheels are fitted, all cars with broad wheels are one line station variant, and cars with narrow wheels are another line station variant, regardless of any other specifications, because the other specifications are not relevant to the wheel line station. Station The line station for which the LSV applies. For Order If the LSV is order-specific, this field displays for which order the LSV is made specific. Note This field is only displayed if the selected LSV is order-specific. Related topics Line station variants and line station orders Process This field is not in use. It is reserved for functionality that is not yet available. Operation The operation linked to the LSV. Operation Variant This field is not in use. It is reserved for functionality that is not yet available. Original Operation If this check box is selected, the operation has not been altered. If this check box is cleared, one of the fields of the assembly operation has been changed. You can only do this if the LSV is order-specific. This check box is used to determine the printing result. When originals must be printed, the operations for which this check box is selected are printed. When differences must be printed, the operations for which this check box is cleared are printed. Related topics Line station variants and line station orders Work Team The team of employees who carry out the operation. Execution Sequence The order in which the operations must be carried out. Instruction If this check box is selected, an instruction text is present. Task An activity to manufacture or repair an item. For example, sawing, drilling, or painting. A task is carried out on a work center, and can be related to a machine. Cycle Time In ERP Enterprise, the time between completion of two separate units of production. For example, the cycle time of motors assembled at a rate of 120 per hour is 30 seconds, or with Machine Occupancy of two, 120 minutes to complete two unites. The cycle time for this machine is 60 minutes; the total time it takes to complete the units is divided by the quantity of units the machine can handle at once. The time required to process a quantity of an item during a certain operation. The quantity for which the cycle time is defined is the routing unit. Cycle time does not include setup time. Cycle Time Unit Hours, minutes or seconds Man Occupation The number of people needed to carry out the operation. This value is retrieved from the line station assignment in Line Assembly Control (LAC). This information is only used in order-based transaction processing. In line-station-based transaction processing, the man occupation is taken from the line-station-level assignment. Machine Occupation The number of machines needed to carry out the operation. This value is retrieved from the line station assignment in Line Assembly Control (LAC). This information is only used in order-based transaction processing. In line-station-based transaction processing, the machine occupation is taken from the line station level assignment. Assembly Parts Click to start the Line Station Variant - Assembly Parts (tiasc2121m000) session. |