| # Clustering Line Station Order - Assembly Part Requirements Parameters The Transaction Processing parameter determines the use of CLSOs. This parameter is defined in the Assembly Control Parameters (tiasc0100m000) session, and can have the following values: Line Station Based Only one CLSO is created for each line station each day. Order Based One CLSO is created for each assembly order. So, in Line Station Based transaction processing mode, a CLSO is used for an entire day. However, the data for each bucket are kept separate, and each bucket gives rise to a separate warehousing order line, for planned stock transactions for the assembly part allocation in Warehousing. You can see that data in the current session. You can see the CLSOs in the Clustered Line Station Orders (tiasc7530m000) session. You can define buckets in the Bucket Definition (tiasl1100m000) session. Note In this session, you see only the assembly parts that have not yet been backflushed. Related topics Assembly control overview Line station variants and line station orders Assembly order costing Assembly backflushing Assembly orders |