| # Work Center Utilization by Week (tisfc1501m000) Use this session to display an overview of capacity utilization for one work center for a week. You can see what orders have been planned, and how much time and materials they are expected to use. Related topics Production orders - functional overview How to calculate available capacity To use an overview session To maintain records in an overview session Shared work centers Work Center The work center for which you want to see a summary of the capacity requirements planned for that week. To see utilization for a shared work center, use the Shared Work Center Utilization (tisfc1510m000) session. Total Hours The total number of man hours for all production orders that are planned to be carried out on the work center. Related topics Calculating man/machine hours Production Year The year for which you want to display data about the planned work center utilization. Normal Capacity The average capacity of a machine or work center that is used as the basis for the capacity utilization. The normal capacity of the persons on the work center is calculated as follows:
    Normal Capacity = Number of Operators * Basic Week Capacity by Resource Unit.
The Number of Operators and the Week Capacity [Hours] are entered in the Work Centers (tirou0101m000) details session. Production Week The week for which you want to see how much capacity has been planned for the work center. Available Capacity Available Capacity Related topics How to calculate available capacity Day The date for which you want to see what demands are planned for the work center. Production Order The production order number. Item The item that is produced in the operation. Item The description of the item produced in the operation. Machine The machine with which the operation is carried out. Quantity Planned The quantity of items you plan to produce in this operation at the work center on this date, including items lost to scrap and low yield. Operation The code of the operation carried out at the work center. Physical Location The location where the order is processed. SFC Order Group The group of orders to which the order belongs. Related topics Order grouping Total Hours The total number of machine hours for all production orders that are planned to be carried out on the work center. Related topics Calculating man/machine hours Normal Capacity The average capacity of a machine or work center that is used as the basis for the capacity utilization. The normal capacity of the machines on the work center is calculated as follows:
    Normal Capacity = Number of Machines * Basic Week Capacity by Resource Unit.
The Number of Machines and the Week Capacity [Hours] are entered in the Work Centers (tirou0101m000) details session. Available Capacity The total capacity in machine hours that are planned to be available on the work center. The available capacity is calculated as follows:
    Number of machines * available number of hours according to the work center calendar (taking into account the capacity percentage defined for the calendar)
Production Planning Starts the Production Planning (tisfc0110m000) session. Build Utilization Starts the Build Utilization (tisfc0201m000) in which you can update the plans from the Enterprise Planning module. All the utilization data is deleted and is regenerated using the production quantity and date data in the Production Planning (tisfc0110m000) session. You must select Automatic in the Update Method Week Utilization field of the Shop Floor Control Parameters (tisfc0100s000) session before you can use this option. |