| # E-Item Revisions by MBC (tiedm3540m000) Use this session to display which E-item revisions are linked to a mass bill of material change (MBC)). You can see details in the E-Item Revisions by MBC (tiedm3540m000) details session. You can link revisions, or delete a link, to an MBC line in the E-Item by MBC (tiedm3122m000) session. Related topics Engineering items To change EBOMs - Automatic procedure Engineering data management summary MBC Number The code of the MBC to which revisions are linked. MBC Number The MBC's status. Engineering Item The E-item whose revisions are linked to the MBC. For more details, double-click the E-item. Description The description or name of the code. Engineering Item Revision The E-item revision, which is linked to the MBC. Status The status of the revision. Related topics Engineering items Effective Date The first day on which a record or a setting is valid. The effective date often includes the effective time. Expiry Date When the revision is no longer valid. Engineer The employee responsible for the revision. E-Item Revision Text If this check box is selected, a text is present. To view the text, click the Text button. Material What the revision is made of, for example paper, plastic, or wood. BOM Quantity The number of manufactured items to which a bill of materials (BOM) applies. The BOM quantity enables you to specify very small item quantities as BOM components. Example You need very small amounts of certain colors to mix one liter of a specific paint, Cotton White. Therefore, a BOM quantity of 1000 liter is defined. The component quantities for the paint can then be as follows:
Paint Cotton White, 1000 liter:
White | 999 liter
Yellow | 0.6 liter
Red | 0.2 liter
Blue | 0.2 liter
Size How large the revision is. For example 200 mm x 1 meter. Unit Set A group of unit codes that can be linked to standard or customized items, or to item defaults. In a unit set, you can indicate the physical quantities that can be used for the item, in which modules, and for what purposes. Norm Standard The company, national or international standard to which the revision conforms (or must conform). For example, ISO 8601, NEN 3140, BS 1383. Unit The physical quantity in which an item or good is managed. For example, a quantity of wood can be expressed as a length by using the unit of one meter, or as a volume by using the unit of one cubic meter. Weight Weight. |