| # Aggregating Estimated Capacity to Project Dependent on the value of the Critical Capacity for Planning field in the Work Centers (tirou0101m000) session, Man Capacity or Machine Capacity is used to calculate the aggregated capacity. You can decide to link activities to the customized operations during the aggregation process. This goes as follows: If the activity code in the Activities (tipcs4101m000) session has not been filled in, or if you indicated that the code can be overwritten, LN first searches for an activity in which the task AND the work center of the activity match the task and the work center of the customized operation. If this activity code is not present, LN searches for an activity in which the task OR the work center of the activity matches with the task or work center of the customized operation. If this activity code is not present, LN searches for an activity in which the main work center of the activity matches the main work center of the customized operation. LN, finally, reports if the customized operation cannot be linked to an activity. Related topics Network planning |