| # Option Combination Lists (tiasl1511m000) Use this session to view lists of option combinations. You can use these lists in the Line Rules (tiasl1570m000) session to define rules stating that certain option combinations must either be sequenced next to each other (clustered), or not sequenced next to each other (blocked). You can define which option combinations are in each list in the Option Combinations List - Option Combinations (tiasl1565m000) session. You can start that session from the appropriate menu. Related topics Assembly control overview Line sequencing and rule types in Assembly Control Option List Code Code of the list of the option combination. Related topics Line station variants and line station orders Option List Code Description of the list of the option combination. Related topics Line station variants and line station orders List Type The option combinations in this list are used in a rule that ensures that they are not sequenced next to each other. Related topics Line sequencing and rule types in Assembly Control Option Combinations Click to stast the Option Combinations List - Option Combinations (tiasl1565m000) session. |