| # Viewing Line Segment - Line Rules In Line Assembly Control (LAC), you can link several rules, each of which is valid for a different date range. You can also link more than one rule to the same segment for the same date range. In that case, if there is a contradiction, the rule with the highest priority takes precedence. You can define rules in the Line Rules (tiasl1570m000) session, or in your configurator package. Related topics Assembly control overview Line sequencing and rule types in Assembly Control |