| # Non-Conformance Material Report Use Non-Conformance Material Report to report and disposition non-conforming material identified during inspection (Quality or Warehouse Inspection) or during the movement of the materials and/or when the material is in stock. The material is inspected to verify that the items conform to the relevant specifications and/or drawings. During the material inspection process, if a non-conformance is detected, the material is immediately isolated. This process is used for various materials, such as purchased materials, materials issued for production orders, finished goods, and materials associated with sales orders. The Non-Conformance Material Report includes materials from the following, regardless of whether the materials were inspected: Purchase Sales Warehouse Transfers SFC Production EP Distribution Storage Inspection To retain the traceability, Infor LN allows you to define a parent child relationship between two NCMRs. If you use Split NCMR, Infor LN refers to the existing NCMR as a parent and the subsequent NCMR as a child. Based on the integration with Warehousing, you can view the NCMR generated for the stockpoint that are blocked in Warehousing. In the Non-Conforming Material Reports (NCMR) (qmncm1100m000) session, the Origin field is set to Warehouse Inventory. |