| # Print Reference Designators by Engineering Bom (tiedm2410m000) Use this session to print reference designators by engineering BOM. Related topics Overview of reference designators Procedure for linking reference designators in the EBOM Reference designators and MBCs Print by Item / Reference Designator The type of report you want to print: Click Print by Item to print a report that lists the reference designators that are linked to a specific engineering item. Click Print by Reference Designator to print a report that lists the engineering items that have BOM lines to which a specific reference designator is linked. From Engineering Item An item in the process of development. You can define multiple revisions of an engineering item. Typically, the most recent revisions are still in a design or test phase, another revision may have been taken into production, and older revisions are obsolete. A normal item can only become revision-controlled when it is copied from the Engineering Data Management module. Engineering Item Revision A version or revised version of an engineering item (E-item) or a revision-controlled item, that is, an item linked to an E-item. Several revisions of an E-item can exist. Example E-item: Mountain bike E-MB01
Revision | Description | Status
--- | --- | ---
A1 | Draft drawing of bike | Not released
A2 | Drawing of bike | Not released
A3 | Parent E-item of bike MB01 | Released
A4 | Obsolete bike | Canceled
Position The number of the EBOM line. Reference Designator Indicates the location to insert a component on an item, for example, where to mount an electronic component on a Printed Circuit Board. Reference designators are often used in electronics, and can originate from a Computer-Aided Design (CAD) station. Related topics Overview of reference designators |