| # Clustering Line Station Order CLSOs are used in assembly part allocation and in backflushing to combine materials for a line-station order (for a day). Parameters The Transaction Processing parameter determines the use of CLSOs. This parameter is defined in the Assembly Control Parameters (tiasc0100m000) session, and can have the following values: Line Station Based Only one CLSO is created for each line station each day. Order Based One CLSO is created for each assembly order. CLSOs are used in assembly part allocation and in backflushing to combine materials for a line station order. A CLSO covers an entire day, in line-station based transaction processing, or an assembly order, in order-based transaction processing. The data for each time bucket is kept seperate. In line-station based transaction processing, each time bucket results in a separated warehousing order line for the assembly part allocation. In order-based transaction processing, an individual warehouse order is generated for each CLSO. Through the appropriate menu you can perform the following actions: Change the status of a CLSO from Closed to Open. Start the Clustered Line Station Order - Assembly Part Requirements (tiasc7140m000) session to view the assembly part requirements for each CLSO. Related topics Line station variants and line station orders Assembly orders |