| # Build Utilization (tisfc0201m000) Use this session to update the calculations of how much you have planned to use machines and work centers, for a selection of variables. Related topics Production orders - functional overview Shared work centers Input / output control Selection Order This field is used to choose the most efficient method to calculate capacity utilization. For example, if you have selected a limited range of work centers to rebuild utilization for, you should select Work Center. If you enter the same value in the From and To fields of any of the selection ranges, LN will select that range in this field, and this field is unavailable. Regenerative Run If this check box is selected, LN recalculates the capacity utilization by deleting the existing data for the selected range and recalculating the data. If you have selected Automatic in either the Update Method Week Utilization field or in the in the Update Method Day Utilization field in the Shop Floor Control Parameters (tisfc0100s000) session, LN calculates the utilization until the end of the period. If this check box is cleared, LN only recalculates the capacity utilization for work centers and machines for which you have changed the planning of orders. LN will only do this if you have selected Manual in either the Update Method Week Utilization field or in the in the Update Method Day Utilization field in the Shop Floor Control Parameters (tisfc0100s000) session. Build Updates the calculations of how much you have planned to use machines and work centers, for your selection. |