| # Noncritical cumulative production lead time Enterprise Planning uses an items noncritical cumulative order lead time (noncritical COLT) to correctly calculate the minimum value of the order horizon. For manufactured items, the noncritical COLT consists of: The lead time of the item itself. The longest noncritical COLT among the item's noncritical components in the BOM. The lead time of the item itself consists of: The order lead time defined in the Items - Production (tiipd0101m000) session. The outbound lead time defined in the Warehouse - Item (whwmd2110s000) session. The safety time defined in the Item - Ordering (tcibd2100s000) session. The extra lead time defined in the Item - Ordering (tcibd2100s000) session. In the Check Horizons (cprpd1200m000) session, you can fill in the following fields to influence the COLT calculation: Additional Lead Time: extra lead time that Enterprise Planning adds to the item's COLT and noncritical COLT. Lead-Time Multiplier: a factor that Enterprise Planning applies to increase the total lead time of the involved item. Related topics Cumulative order lead times and horizons Cumulative production lead time |