| # Manufacturing operations When Infor LN Quality is implemented for routing operations, Infor LN creates inspection orders for each operation. These inspection orders specify the tests for the subassemblies produced. Possible scenarios to implement quality for the routing operations: The subassemblies are inspected, but the operations are not affected by the inspection orders (method A). You must inspect the subassemblies, before you can report an operation completed. However, you can report the quantity completed or rejected, irrespective of the results of the tests (method B). You must inspect the subassemblies, before you can report quantities completed or rejected. The inspections result in recommendations for the quantities completed and rejected (method C). You must inspect the subassemblies, before you can report quantities completed or rejected. The results of the inspections determine the quantity completed and rejected. You cannot modify these quantities (method D). Consequences for reporting completed The method you select determines the usage of the following fields in the Report Operations Completed (tisfc0130m000) session: Quantity Completed Rejected Quantity To Inspect You must enter the data in the Quantity Completed field and the Rejected field, only when you select method A & B. If the subassemblies must be inspected before reporting the quantities complete or rejected (method C and D): The Quantity Completed field and the Rejected field are blocked. You can enter the data in the Quantity To Inspect field. Infor LN populates the Quantity Completed field and Rejected field with the inspection results when the inspection order is processed. If you use method C, you can modify the Quantity Completed field and Rejected field, after you close the inspection order. Note If you select method A, and want to modify the quantities completed or rejected, after you have closed the inspection order, Infor LN asks you if the inspection order must be reopened. If you select method B, C, or D, and you want to modify the quantities completed or rejected, after you closed the inspection order, Infor LN generates a new inspection order. Related topics Integration with SFC Blocking operations Defining blocking reasons for Quality |