| Serial End Item - As-Built Headers (timfc0110m000) |  |
| Use this session to maintain and display the serialized end items built in the Assembly Control (ASC) module or the Shop Floor Control (SFC) module. For every individual serialized item of an assembly order or a production order a line is present in this session. For example, for an ordered quantity of six items, six lines are present in this session, each line having a serial number that is a unique identification of a single physical item. An example of a serial number is the Vehicle Identification Number (VIN) of a car. If you select an item in this session, and you click As-Built Components from the appropriate menu, the serialized components of each serialized end item are displayed in the Serial End Item - As-Built Components (timfc0111m000) session. The serialized end item and its serialized components form together the as-built structure, which enables you to track order data, and to investigate which components are in each individual end item. Shop Floor Control (SFC) The moment you can display the as-built structure of a serialized item produced in Shop Floor Control depends on the Moment of Generating Serial Numbers field in the Shop Floor Control Parameters (tisfc0100s000) session. At various moments, you can enable ERP LN to generate serial numbers based on a mask. If the mask is not present, you must insert serial numbers manually. Assembly Control (ASC) Serial numbers can be generated when you have confirmed the line sequence in Assembly Control. You can then display the as-built structure of the item. Note You can only delete an as-built serial item if the serial status is Created. Related topics Overview of serialized items Serialized items in Manufacturing To define a mask
Fields | Description
Production / Assembly Order | The production order or the assembly order for which the serialized item is produced.
Item | The parent item for which the serialized item is derived.
Item Effectivity Unit | The item's effectivity unit.
Serial Number | The unique identification of a single physical item. ERP LN uses a mask to generate the serial number. The serial number can consist of multiple data segments that represent, for example, a date, model and color information, sequence number, and so on. Serial numbers can be generated for items and for tools.
Lot Code | A number of items produced and stored together that are identified by a (lot) code. Lots identify goods.
Serial Status | The status of the end item's serial number. Allowed values Possible Values Related topics Working with serialized items in Manufacturing
Valid | If this check box is selected, the as-built structure is complete. An as-built structure is complete when serial numbers are present for serialized components, and lot numbers for lot-controlled (serialized) items. ERP LN automatically checks the completeness of the as-built structure when the serial status changes (manually or automatically) from Created or Rejected to Assigned. If an as-built structure is not valid, you cannot copy the as-built structure to an as-maintained structure in the Create Physical Breakdown Structure (tscfg2210m000) session. Furthermore, if the Check as-built serials field in the Inventory Handling Parameters (whinh0100m000) session is Warn or Block, the item cannot be shipped. Related topics Working with serialized items in Manufacturing
Rework Order | If rework exists for the serialized item, this field displays the rework order number. Related topics Rework orders
Commands | Description
As-Built Components | ERP LN starts the Serial End Item - As-Built Components (timfc0111m000) session. In this session you can display the components of the serialized item.
Generate Serial Numbers | If you click this button, ERP LN generates serial numbers for the items produced for the assembly order.
Validate | Click to check whether the as-built structure is complete. An as-built structure is complete when serial numbers are present for serialized components, and lot numbers for lot-controlled (serialized) items. An as-built structure is incomplete when serial numbers and/or lot numbers are missing.