| Test Data History by Serial Number (qmptc3516m000) |  |
| Use this session to display the test data by serial number. The data was previously entered in the Sample - Test Data by Serial Number (qmptc1116m000) details session. Test data lines were created for each position of the inspection order. Example If an inspection order has four positions with a characteristic, four lines are generated. Note The Sample Test Data by Characteristic History (qmptc3515m000) session displays test data that is entered by characteristic. The session in which you enter your test data depends on how you set the Enter Test Data by parameter in the Quality Management Parameters (qmptc0100m000) session. Related topics Standard inspections
Fields | Description
Inspection Order | The code of the inspection order.
Sample | A small quantity that is drawn from the total (order) quantity and which represents the order quantity's quality.
Aspect | A part of an item. For example, a bolt can have the aspects head and tail. An aspect can have one or more characteristics. For example, a head can have a diameter and a length, and a tail can have a diameter and a color.
Serial Number | A unique number generated by ERP LN to distinguish between the different measurements you can do in one sample quantity. The number of measurements is based on the test quantity.
Example
Sample quantity | 100 pieces
Test quantity | 20 pieces
Explanation: You need to do five tests on twenty pieces to get a sample quantity of one hundred pieces (100/20=5). Consequently, five test lines are generated, with each an unique serial number. Note The total number of serial numbers cannot exceed the value of the sample quantity divided by the test quantity
Charact. | A reference to a particular quality or distinctive mark of an item or an item part/component. For example, diameter, length, weight.
Position | The position number represents a characteristic that is measured. The measured value is entered as test data in the Sample Test Data (qmptc1115m000) session, or the Sample - Test Data by Serial Number (qmptc1116m000) session.
Item | In ERP LN, the raw materials, subassemblies, finished products, and tools that can be purchased, stored, manufactured, sold, and so on. An item can also represent a set of items handled as one (kit), or exist in multiple product variants. You can also define nonphysical items, which are not held in inventory but can be used to post costs or to invoice services to customers. Examples of nonphysical items: Cost items (for example, electricity) Service items Subcontracting services List items (menus/options)
Method | The type of characteristic value, or the way in which the characteristic value is calculated.
Test Date | The date and time when the test took place.
Measurement Value | The result of the test. A numeric value is displayed if you selected Quantitative in the Result Type field, and if the Characteristic Type field was not set to Option. If an algorithm was specified for the inspection order line, the algorithm calculated the numeric value that is displayed in this field.
Unit | The unit in which the test results are defined or calculated. Note This field does not apply if you entered Option in the Characteristic Type field.
Option Set | A group of possible values of a characteristic. For each value (option) you can indicate whether it is acceptable or not. The options blue and red form an option set Example
Characteristic | pH value
Test | Litmus test
Options | blue = acceptable
red = not acceptable
Option | The option that was found. Note Depending on what you entered in the Option Type field in the Options (qmptc0114m000) session, the option is either Acceptable or Not Acceptable.
Test Area | The physical location where tests take place.
Employee | The person that performs the test on this characteristic.
Instrument | The default instrument used to measure the characteristic.
Result | The result of the inspection. Note ERP LN automatically generates a value, depending on the quality limits that you defined in the Quality ID - Characteristics (qmptc0115m000) session and/or in the Options (qmptc0114m000) session.