| Instructions by Operation(Step) (tisfc0142m000) |  |
| Use this session to display and modify the instructions that are linked to an operation/ operation step combination for a specific production order. If you want to display all instructions linked to a specific production order, use the Instructions by Production Order (tisfc0141m000) session. Performance aspects The settings in this session could affect system performance and database growth. For more information, refer to Micro routing. Related topics Microrouting
Fields | Description
Production Order | An order to produce a specified quantity of an item on a specified delivery date.
Operation | One of a series of steps in a routing that are carried out successively to produce an item. The following data is collected during a routing operation: The task. For example, sawing. The machine used to carry out the task (optional). For example, sawing machine. The place where the task is carried out (work center). For example, woodwork. The number of employees required to carry out the task. This data is used to compute order lead times, to plan production orders and to calculate cost prices.
Operation Step | The operation step to which instructions can be linked. If the value of this field is is 0 (zero), the instruction is directly linked to the operation.
Instructions | The instruction that is linked to the operation/ operation step combination, and which is printed on the production order documents. If the Operation Step field is 0 (zero), the instruction is only linked to the operation. The instruction can be a document identification that refers to a document containing specific instructions. These instruction documents can be displayed on the computer screen or on printed paper.
Production Order | The status assigned to a production order, which indicates how far a production order has been processed. For example, Planned, Documents Printed, or Released.
Operation | The status assigned to an operation. For example, Planned, Ready to Start, or Completed. This status indicates how far an operation has proceeded.