| Print Assembly Part Requirements (tiasc7440m000) |  |
| Use this session to print the assembly parts requirements. Select at least one of the following check boxes to print the assembly part requirements: To be Allocated. To be Backflushed. According to your selection the requirements for parts to be allocated, or for parts to be backflushed, or for both these options are printed. Parameters Assembly part requirements are stored by Clustered line-station orders (CLSOs). CLSOs are used in assembly-part allocation and in backflushing to combine materials for a line station. However, the content of CLSOs varies, depending on whether you work line station based or order based: Line Station Based A CLSO is for an entire day. Each time bucket (day) results in a separate warehousing order line for the assembly part allocation. Order Based A CLSO is for an assembly order. A separate warehouse order is generated for each CLSO. These options are defined by the Transaction Processing parameter, defined in the Assembly Control Parameters (tiasc0100m000) session. Note You can view the CLSOs in the Clustered Line Station Orders (tiasc7530m000) session. You can define buckets in the Bucket Definition (tiasl1100m000) session. Related topics Assembly control overview Line station variants and line station orders Assembly order costing Assembly backflushing Assembly orders |