| Item Storage Inspections History (qmptc3502m000) |  |
| Use this session to select an item for which you want to select storage inspection orders. This session is used only for selection purposes in the Delete Inspection History (qmptc3210m000) session, the Print Inspection Plan History (qmptc3401m000) session, and the Print Inspection Result History (qmptc3405m000) session. Related topics Storage inspections
Fields | Description
Item | In ERP LN, the raw materials, subassemblies, finished products, and tools that can be purchased, stored, manufactured, sold, and so on. An item can also represent a set of items handled as one (kit), or exist in multiple product variants. You can also define nonphysical items, which are not held in inventory but can be used to post costs or to invoice services to customers. Examples of nonphysical items: Cost items (for example, electricity) Service items Subcontracting services List items (menus/options) Note Standard items are expressed in an item code. Segmented items consist of a project code segment and an item base segment (the item code of the customized item). The segments an item can consist of are defined in the Item Code Segmentation (tcibd0500m000) session.
Sequence | The sequence number of the inspection order on the basis of which characteristics are tested on different samples.
Quantity Ordered | The quantity for which the inspection is required. Consequently, the result of the inspection order concerns the quality of this quantity.
Recommended | The quantity to be accepted, as recommended by the Quality package, expressed in the inventory unit. The total of all sample quantities which passed the tests successfully. Note This quantity is automatically updated by use of the Process Inspection Orders (qmptc1204m000) session.
Recommended | The quantity to be rejected as recommended by the Quality package, expressed in the inventory unit. The total of all sample quantities which do not have the required quality level. Note This quantity is automatically updated by use of the Process Inspection Orders (qmptc1204m000) session.
Actual | The actual quantity that is accepted, expressed in the inventory unit. The actual quantity can be adjusted until the inspection order is closed. Storage inspections are always only recommended. All inventory of the storage inspection order will be unblocked after closing the inspection.
Actual | The actual quantity that is rejected, expressed in the inventory unit. The actual quantity can be adjusted until the inspection order is closed. Storage inspections are always only recommended. All inventory of the storage inspection order will be unblocked after closing the inspection.
Completion Date | The date on which all inspection order lines are completed. This date is updated automatically in the Complete/Process Inspection Orders (qmptc1202m000) session, and cannot be entered manually.
Recommended Quantity Destroyed | The total quantity destroyed during a destructive test, expressed in the order unit. The quantity destroyed is equal to the sample size of the inspection orders that are tested by means of destructive tests. The quantity destroyed does not have any impact on the accepted or rejected quantities. ERP LN only calculates the quantity that is destroyed according to the test. Note This quantity is automatically updated in the Process Inspection Orders (qmptc1204m000) session.