| Work Center Input/Output Control (tisfc3510m000) |  |
| Use this session to see a summary of the planned and actual input and output values for a work center. You can start the following sessions from the appropriate menu: Generate Work Center Input/Output Control (tisfc3210m000) Delete Work Center Input/Output Control (tisfc3212m000) Note If you want to see input/output data for a machine, use the Machine Input/Output Control (tisfc3520m000) session. Related topics Input / output control
Fields | Description
Work Center | The work center for which you want to compare actual and planned inputs and outputs. Note that you can only see data for work centers whose Critical in Planning check box is selected in the Work Centers (tirou0101m000) session.
Description | The work center for which you want to compare actual and planned inputs and outputs. Note that you can only see data for work centers whose Critical in Planning check box is selected in the Work Centers (tirou0101m000) session.
Lead Time | The desired queue that is defined for the work center in the Work Centers (tirou0101m000) details session.
Planned Input | The total input quantity of a work center/machine for operations that is planned to be Ready to Start during the target period.
Actual Input | The total input quantity of a work center/machine for operations that are Ready to Start during the target period.
Input Cumulative Deviation | The sum of the differences between the planned input and the actual input for the current target period and all the target periods before the current one for which you have data.
Planned Output | The total output quantity that you plan to report complete, for operations at a work center/machine during the target period.
Actual Output | The total output quantity that is reported complete, for operations at a work center/machine during the target period. The value of the actual output depends, among other things, on the setting of the Include Partial Completions (Default) check box in the Generate Work Center Input/Output Control (tisfc3210m000) session.
Output Cumulative Deviation | The sum of the differences between the planned output and the actual output for the current target period and all the target periods before the current one, for which you have data.
Planned Queue | The planned input minus the planned output of a work center/machine.
Actual Queue | The actual input minus the actual output of a work center/machine. Note that the queue includes active operations as well as operations waiting to be carried out.
Queue Deviation | The difference between the planned queue and the actual queue on the generation date, that is actual queue minus planned queue.
Desired Queue Deviation | The actual queue minus the desired queue.
Available Capacity | The total capacity available, for either a day or a week, usually based on the work center calendar.
Demonstrated Load Factor | Combined efficiency and utilization. The ratio of actual output to available capacity, for an operation performed at a given work center or machine.
Ending Date | The last day of the target period.
Number of Operators | The number of operators that is available on the work center.
Man Hours | The number of man hours that are desired on the work center, given the desired queue. Man hours = Number of operators on the work center * Desired queue
Number of Machines | The number of machines that is available on the work center.
Machine Hours | The number of machine hours that are desired on the work center, given the desired queue. Machine hours = Number of machines on the work center * Desired queue
Planned Input | The total input quantity of a work center/machine for operations that is planned to be Ready to Start during the target period.
Actual Input | The total input quantity of a work center/machine for operations that are Ready to Start during the target period.
Input Cumulative Deviation | The sum of the differences between the planned input and the actual input for the current target period and all the target periods before the current one for which you have data.
Planned Output | The total output quantity that you plan to report complete, for operations at a work center/machine during the target period.
Actual Output | The total output quantity that is reported complete, for operations at a work center/machine during the target period.
Output Cumulative Deviation | The sum of the differences between the planned output and the actual output for the current target period and all the target periods before the current one, for which you have data.
Planned Queue | The planned input minus the planned output of a work center/machine.
Actual Queue | The actual input minus the actual output of a work center/machine. Note that the queue includes active operations as well as operations waiting to be carried out.
Queue Deviation | The difference between the planned queue and the actual queue on the generation date, that is actual queue minus planned queue.
Desired Queue Deviation | The actual queue minus the desired queue.
Available Capacity | The total capacity available, for either a day or a week, usually based on the work center calendar.
Demonstrated Load Factor | Combined efficiency and utilization. The ratio of actual output to available capacity, for an operation performed at a given work center or machine.