| Process backflushed materials |  |
| ERP LN backflushes the materials linked to the operations for which quantities are reported as completed. If a production order has no operations, ERP LN backflushes all materials. For details about the calculation of the quantities to issue through backflushing, see Calculate backflush quantity. You can see the result of backflushing materials in the Production Orders (tisfc0101s000) session. ERP LN subtracts the backflushed material quantity from the Subsequent Delivery field and adds the same quantity to the To Issue field. The correspondig warehousing order is immediately initiated. Note ERP LN does not decrease the value of the Subsequent Delivery field below zero. ERP LN also prints the results of backflushing materials in a report. Related topics Backflushing procedure Link materials to operations Calculate backflush quantity Overview of material issue Backflushing |