| Utilization by Critical Option Combination (tiasl3510m000) |  |
| Use this session to view the number of actual orders and the maximum number of orders on an assembly line for a given date, for option combinations that are used for line mix rules. For more information, see the Line Rules (tiasl1570m000) session. You can view this data as a graph with the Assembly Line - Line Utilization - Chart (tiasl3700m000) session. Related topics Assembly line station utilization
Fields | Description
Assembly Line | A set of consecutive line stations in which FAS (Final Assembly Schedule) items are manufactured. The items are manufactured by passing the items from line station to line station and by carrying out operations at each line station. An assembly line is subdivided into a number of line segments separated by buffers. An assembly line can be either a main line or a supplying line.
Date | The planned offline date for the orders.
Option Combination | A specific combination of product options, for example, color or style, that are related to an assembly order. Each option combination is either a single option, or a combination of other option combinations.
Option Combination | A specific combination of product options, for example, color or style, that are related to an assembly order. Each option combination is either a single option, or a combination of other option combinations.
Actual Number of Orders | The number of orders planned for the option combination.
Maximum Number of Orders | The maximum number of orders possible for the option combination. This is determined by the mix rules defined for the combination in the Line Rules (tiasl1570m000) session.